**CP135**

* 3.2M pixel CMOS image sensor
* Focus: Manual
* Frame Rate: 24 frames per second
* Zoom: 16X Total Zoom (2X AVerZoom™ + 8X Digital Zoom)
* Image Rotation: Camera Head 0° / 90° / -90°
* Capture Mode: Single/Continuous (up to 80 images; 3M each)
* Shooting Area: A4 Landscape
* Output Resolution: up to HD 720p (1280 x 720)
* Add-on Features: AVerPresenter, Split Screen, Picture-in-Picture
* Light Source: Embedded LED Light
* Remote Control
* Connectivity: RGB input and output, S-Video output, Composite Video output
* USB 2.0 port (PC Camera/Built-in image download)
* Operating Dimension: 180mm x 480mm x 504mm
    Folded Dimension: 230mm x 340mm x 61mm
* Weight: 2.4kg
* Software Version: AVer+ 1.3 (compatible with PC and Mac)
* Patent No.: Taiwan I276904, Japan 3122844
* Compliance: FCC, CE, RoHS