**AVerVision SPB series**

* 5M pixel CMOS sensor
* Focus: Auto/Manual
* Frame Rate: 30 frames per second
* Zoom: 160X Total Zoom (20X AVer**®**Optical Zoom + 8X Digital Zoom)
* Image Rotation: Electronic Rotation 0°/ 90° / 180°/270°/ 360°
* Capture Mode: Single/Continuous (up to 80 images)
* Shooting Area: 310mm X 233mm
* Output Resolution: Support HD 1080p (1920x1080)
* Add-on Features: AVerPresenter, PIP, Split Screen
* Embedded LED Light module
* Light Box Size: 5" x 4"
* Connectivity: DVI-I output,VGA input and output, S-Video output, Composite Video output, RS-232
* USB 2.0 port (USB Camera/Built-in image download)
* Memory Card Slot: supporting SD card
* Operating Dimension: 480mm x 380mm x 505 mm  
  Folded Dimension: 480mm x 380mm x 150mm
* Weight: 7kg
* Software Version: AVerVision 3.x for PC; AVerVision 2.x for MAC
* Patent No.: Taiwan 276904 317592 311053 290434 1264977 125702 M334949  
  Japan 3122844
* Compliance : FCC, CE, RoHS